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Quick Start Guide

Overview
[image: ]The LAN/WAN Connection configures the Cradlepoint S450 so that the built-in Ethernet port provides the local LAN connection, while a USB-to-Ethernet adaptor provides the wired WAN/Internet connection.
Additional Required Equipment
AES Part Number: 7177-RT-ETH USB Ethernet Adaptor, Ethernet cables.

Installation Instructions

1. Install the USB Ethernet adaptor. Power down the S450 and plug the USB-to-Ethernet adaptor directly into the S450 USB port. Connect the WAN/network Ethernet cable to the USB adaptor. 

2. Connect the Subscriber. Connect the Subscriber to the S450's built-in Ethernet/PoE port.

3. Power up the S450. Apply power and allow the router to complete its boot sequence.

4. Verify the WAN connection. In NetCloud Manager or the S450 local management interface, verify that the USB Ethernet connection appears as a WAN interface and has received the expected IP address from the upstream network.

5. Verify the LAN connection. Confirm that the built-in Ethernet port is assigned to the LAN. The connected local device should receive an IP address from the S450's DHCP server unless you have intentionally configured static addressing.

6. Configure connection priority if cellular backup is being used. If the goal is wired WAN with cellular failover, configure the connection priority so that the USB Ethernet WAN is preferred and the S450's cellular modem is secondary:
When the wired WAN is available, traffic uses the USB Ethernet connection. If that connection fails, the S450 can route traffic over cellular. When the primary WAN becomes available again, the router can return traffic to the preferred connection.

7. Test the installation. With the USB WAN connected, verify that the LAN device can reach the required network or Internet destination. Then disconnect the Ethernet cable from the USB adaptor and verify cellular failover, if configured. Reconnect the USB WAN and confirm that the router returns to the wired connection.
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